R\_BP:

enable

configure terminal

hostname R\_BP

interface GigabitEthernet0/0

ip address 8.8.0.1 255.255.0.0

no shutdown

exit

ip route 0.0.0.0 0.0.0.0 8.8.8.8